[Back to GRAPHICS SWAG index] [Back to Main SWAG index] [Original]

    { From: 9308920@info.umoncton.ca (DEGRACE KEITH) }

    var
      c, x, y : byte;

    procedure setrgb(c, r, g, b : byte);
    begin
      port[$3c8] := c;   { g'day, this is a probably the most simple version   }
      port[$3c9] := r;   { of fire that you will ever see in pascal. i wrote   }
      port[$3c9] := g;   { the code in pascal so it's slow and choppy, i have  }
      port[$3c9] := b;   { another version in asm. and it's faster. anyways if }
    end;                 { you have any critics or question on this code, just }
                         { e-mail me at ekd0840@bosoleil.ci.umoncton.ca. or    }
    begin                {              9323767@info.umoncton.ca               }
      randomize;         {  note : I have code for all kinds of stuff (that I  }
      asm   mov ax, 13h  {         wrote of course), if you want something     }
            int 10h      {         e-mail me (i never get mail), maybe i have  }
      end;               {         what you want.                              }
      for x := 1 to 32 do{                               keith degr�ce         }
       begin             {                               moncton, n.-b. canada }
        setrgb(x, (x shl 1)-1, 0, 0 );
        setrgb(x+32, 63, (x shl 1)-1, 0 );
        setrgb(x+64, 63, 63, (x shl 1)-1 );
        setrgb(x+96, 63, 63, 63 );
       end;
      repeat
       for x := 0 to 159 do
        begin
         for y := 30 to 101 do
          begin
           c := (mem[$a000:(y shl 1)*320+(x shl 1)]+
                 mem[$a000:(y shl 1)*320+((x+1) shl 1)]+
                 mem[$a000:(y shl 1)*320+((x-1) shl 1)]+
                 mem[$a000:((y+1) shl 1)*320+((x+1) shl 1)]) shr 2;
           if c <> 0 then dec(c);
           memw[$a000:(((y-1) shl 1)*320+(x shl 1))] := (c shl 8) + c;
           memw[$a000:(((y shl 1)-1)*320+(x shl 1))] := (c shl 8) + c;
          end;
         mem[$a000:(y shl 1)*320+(x shl 1)] := random(2)*160;
        end;
      until port[$60] < $80;
      asm  mov ax, 3
           int 10h
      end;
    end.

[Back to GRAPHICS SWAG index] [Back to Main SWAG index] [Original]